# Introduction

# Requirements

Motor will be designed for a high torque direct drive application.

Rated Speed: 600 rpm

Rated Torque: 250 Nm

Rated Power: 22 kW

Max outer diameter: 400mm

Supply: Inverter fed from 400 V three phase grid

# Analytical Calculations

Firstly, motor dimensions should be calculated analytically. Analytical calculations provide a starting point for FEA and optimization steps.

## Supply and Drive

Motor driver will be supplied from 400V grid. However, it cant be used directly since variable frequency drive will be used. In order to use a vfd, supply should be rectified at first. There are two options. Firstly, diode rectifier can be used. Six diodes with large bus capacitors would do the job. Secondly, an active rectifier can be utilized.

When diode rectifier is used, initial cost is lower. However, diode rectifiers need a large bus capacitor in order to reduce voltage ripple. Additionally, current ripple high and this effects the other grid connected devices nearby. Moreover, since power factor is not controlled, more current is drawn for the same power. Lastly, when a diode rectifier is used, energy can only flow from grid to the DC side, can’t flow back.

When an active rectifier is used, initial cost is higher since there are additional switching devices and controllers. However active rectifier provides in smaller bus capacitor, bidirectional energy flow, reduced grid current and less harmonic disturbance on the grid.

Because of those reasons active rectifier will be used. The simplest method is to use a three phase rectifier with additional LCL filters on the phase connections. This topology results in boost type pfc. In a boost type pfc, output voltage is larger than the input voltage. Also output voltage can be regulated by controlling the transistors.

Now motor voltage can be determined. Input voltage is 400Vrms. Since this voltage is not always constant, limit situations should be considered. Assuming 400V+-15%, max voltage is 460V rms.

Since rectifier is a boost type pfc, minimum regulated output voltage should be 650V for constant DC bus voltage.

SVPWM will be used on the inverter side.

## Motor Current and Wire

Since motor power and voltage is known, phase current can be found.

Taking j = 6 A/mm^2

Using a wire would result in 2.6 mm diameter wire. It is impractical to wing thick cables since bending becomes more and more difficult. Because of that two wires in parallel can be used.

**Chosen wire:** 2x 1.8 mm diameter copper wire

## Pole-Slot Number, Dimensions

# FEA Modelling

# Comparison and Discussion

# Conclusion